ECC Recommendation (14)06

Implementation of Fixed Service Point-to-Point narrow channels (3.5 MHz, 1.75 MHz, 0.5 MHz, 0.25 MHz,
0.025 MHz) in the guard bands and center gaps of the lower 6 GHz (5925 to 6425 MHz) and upper 6 GHz
(6425 to 7125 MHz) bands

**Approved 19 September 2014**

**Ammended May 2015**

# introduction

ECC Report 215 provides the technical feasibility of introducing narrow channel spacings in guard bands and center gaps of Fixed Service channel arrangement defined in ERC/REC 14-01 (5925-6425 MHz) and ERC/REC 14-02 (6425-7125 MHz). This Recommendation provides options for administrations consideration.

# ECC recommendation (14)06 of 19 September 2014 Implementation of Fixed Service Point-to-Point narrow channels (3.5 MHz, 1.75 MHz, 0.5 MHz, 0.25 MHz, 0.025 MHz) in the guard bands and center gaps of the lower 6 GHz (5925-6425 MHz) and upper 6 GHz (6425-7125 MHz) bands Amended 8 May 2015

“The European Conference of Postal and Telecommunications Administrations,

*considering*

1. ERC/REC 14-01 defines channels arrangements for high capacity analogue and digital radio-relay systems operating in the band 5925 -6425 MHz;
2. that ERC/REC 14-02 defines channels arrangements for high, medium and low capacity digital fixed service systems operating in the band 6425-7125 MHz;
3. that the whole band from 5925 to 7125 MHz is allocated in the CEPT and ITU to the fixed service on a primary basis;
4. there are technical and economic advantages in adopting harmonized channel plans which favors equipment development;
5. that ECC Report 215 provides the technical feasibility of introducing narrow channel spacing (25 kHz to 3.5 MHz) in guard bands and center gaps of FWS channel arrangements at 6 GHz;
6. that ECC Report 215 demonstrates that the 6 GHz band is suitable for introducing narrow channels without causing harmful interferences to other services with appropriate mitigation techniques ensuring compatibility between fixed links and satellite services;
7. that some administrations use other FS applications different to radio-relay systems in frequency bands 5925- 6425 MHz and 6425-7125 MHz, and therefore some additional measures for coordination in cross border areas may be required;

*recommends*

1. that administrations wishing to implement narrow channels in the lower part of the 6 GHz band, should refer to the channel arrangement described in Annex 1 (and illustrated in Annex 3);
2. that administrations wishing to implement narrow channels in the upper part of the 6 GHz band, should refer to the channel arrangement described in Annex 2 (and illustrated in Annex 3).

*Note:*

*Please check the Office documentation database http://www.ecodocdb.dk for the up to date position on the implementation of this and other ECC Recommendations.*

1. IMPLEMENTATION OF NARROW CHANNELS in The guard bands and center gap of the 5925-6425 MHz band
	1. DERIVATION OF RADIO FREQUENCY CHANNELS

The radio frequency channel arrangement for carrier spacings of 3.5 MHz, 1.75 MHz, 0.5 MHz, 0.25 MHz and 0.025 MHz shall be derived as follows:

Let

f0 be the frequency (MHz) of the center of the band of frequencies occupied, f0 = 6302.4 MHz;

fn be the center frequency (MHz) of one radio-frequency channel in the lower half of the band;

fn’ be the center frequency (MHz) of one radio-frequency channel in the upper half of the band;

then the frequencies (MHz) of individual channels are expressed by the following relationships:

1. for systems with a carrier spacing of 3.5 MHz:

lower half of the band: fn = f0 – 134.405 + 3.5 n

upper half of the band: fn’ = f0 + 120.403 + 3.5 n where n = 1, 2, 3.

1. for systems with a carrier spacing of 1.75 MHz:

lower half of the band: fn = f0 – 133.53 + 1.75 n

upper half of the band: fn’ = f0 + 121.278 + 1.75 n where n = 1, 2, 3, 4, 5, 6.

1. for systems with a carrier spacing of 0.5 MHz:

lower half of the band: fn = f0 – 132.905 + 0.5 n

upper half of the band: fn’ = f0 + 121.903 + 0.5 n where n = 1, 2…..20, 21.

1. for systems with a carrier spacing of 0.25 MHz:

lower half of the band: fn = f0 – 132.78 + 0.25 n

upper half of the band: fn’ = f0 + 122.028 + 0.25 n where n = 1, 2…..41, 42.

1. for systems with a carrier spacing of 0.025 MHz:

lower half of the band: fn = f0 – 132.6675 + 0.025 n

upper half of the band: fn’ = f0 +122.1405 + 0.025 n where n = 1, 2…..419, 420.

Table 1: Calculated parameters according to Recommendation ITU-R F.746

| **XS****(MHz)** | **n** | **f1****(MHz)** | **fn****(MHz)** | **f1’****(MHz)** | **fn’****(MHz)** | **YS (MHz)** | **DS (MHz)** |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 3.5 | 1…3 | 6171.495 | 6178.495 | 6426.303 | 6433.303 | 247.808 | 254.808 |
| 1.75 | 1…6 | 6170.62 | 6179.37 | 6425.428 | 6434.178 | 246.058 | 254.808 |
| 0.5 | 1..….21 | 6169.995 | 6179.995 | 6424.803 | 6434.803 | 244.808 | 254.808 |
| 0.25 | 1…...42 | 6169.87 | 6180.12 | 6424.678 | 6434.928 | 244.558 | 254.808 |
| 0.025 | 1….420 | 6169.7575 | 6180.2325 | 6424.5655 | 6435.0405 | 244.333 | 254.808 |

XS Separation between centre frequencies of adjacent channels;

YS Separation between centre frequencies of the closest go and return channels;

Z1S Separation between the lower band edge and the centre frequency of the first channel;

Z2S Separation between centre frequencies of the final channel and the upper band edge;

DS Duplex spacing (fn’ - fn).

**6167.575**

**6440 MHz**

244.308 MHz

2.17

MHz

3 x 3.5 MHz

3 x 3.5 MHz

4.947

MHz (note 1)

a) 3.5 MHz channels

c) 0.5 MHz channels

244.308 MHz

2.17

MHz

21 x 0.5 MHz

21 x 0.5 MHz

4.947

MHz (note 1)

d) 0.25 MHz channels

244.308 MHz

2.17

MHz

42 x 0.25 MHz

42 x 0.25 MHz

4.947

MHz (note 1)

e) 0.025 MHz channels

244.308 MHz

2.17

MHz

420 x 0.025 MHz

420 x 0.025 MHz

4.947

MHz

b) 1.75 MHz channels

244.308 MHz

2.17

MHz

6 x 1.75 MHz

6 x 1.75 MHz

4.947

MHz (note 1)

1. Occupied spectrum

Note: This figure depicts the occupied spectrum by the narrow channels in the lower part of the band simultaneously implemented with 40 MHz bandwidth channels in the U6 band. In case of implementation of 30 MHz bandwidth channels in the U6 band, 5 MHz must to be added to the upper guard band (e.g. 9.947 MHz instead of 4.947 MHz).

1. IMPLEMENTATION OF NARROW CHANNELS IN THE GUARD BANDS AND CENTER GAP OF THE 6425 - 7125 MHz Band
	1. Implementation of narrow channels (40 MHz channels)
		1. Derivation of radio frequency channel

The radio frequency channel arrangement for carrier spacings of 3.5 MHz,, 1.75 MHz, 0.5 MHz, 0.25 MHz and 0.025 MHz shall be derived as follows:

Let

f0 be the frequency (MHz) of the center of the band of frequencies occupied, f0 = 6 941.25 MHz;

fn be the center frequency (MHz) of one radio-frequency channel in the lower half of the band;

fn’ be the center frequency (MHz) of one radio-frequency channel in the upper half of the band;

then the frequencies (MHz) of individual channels are expressed by the following relationships:

a) for systems with a carrier spacing of 3.5 MHz:

lower half of the band: fn = f0 – 180 + 3.5 n

upper half of the band: fn’ = f0 + 162.5 + 3.5 n where n = 1, 2, 3, 4.

b) for systems with a carrier spacing of 1.75 MHz:

lower half of the band: fn = f0 – 179.125 + 1.75 n

upper half of the band: fn’ = f0 + 163.375 + 1.75 n where n = 1, 2, ...7, 8.

d) for systems with a carrier spacing of 0.5 MHz:

lower half of the band: fn = f0 – 178.5 + 0.5 n

upper half of the band: fn’ = f0 + 164 + 0.5 n where n = 1, 2…..27, 28.

e) for systems with a carrier spacing of 0.25 MHz:

lower half of the band: fn = f0 – 178.375 + 0.25 n

upper half of the band: fn’ = f0 + 164.125 + 0.25 n where n = 1, 2…..55, 56.

f) for systems with a carrier spacing of 0.025 MHz:

lower half of the band: fn = f0 – 178.2625 + 0.025 n

upper half of the band: fn’ = f0 + 164.2375 + 0.025 n where n = 1, 2…..559, 560.

Table 2: Calculated parameters according to Recommendation ITU-R F.746

| **XS****(MHz)** | **n** | **f1****(MHz)** | **fn****(MHz)** | **f1’****(MHz)** | **fn’****(MHz)** | **YS (MHz)** | **DS (MHz)** |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 3.5 | 1…4 | 6764.75 | 6775.25 | 7107.25 | 7117.75 | 332 | 342.5 |
| 1.75 | 1…8 | 6763.875 | 6776.125 | 7106.375 | 7118.625 | 330.25 | 342.5 |
| 0.5 | 1..….28 | 6763.25 | 6776.75 | 7105.75 | 7119.25 | 329 | 342.5 |
| 0.25 | 1…...56 | 6763.125 | 6776.875 | 7105.625 | 7119.375 | 328.75 | 342.5 |
| 0.025 | 1….560 | 6763.0125 | 6776.9875 | 7105.5125 | 7119.4875 | 328.525 | 342.5 |

XS Separation between centre frequencies of adjacent channels;

YS Separation between centre frequencies of the closest go and return channels;

Z1S Separation between the lower band edge and the centre frequency of the first channel;

Z2S Separation between centre frequencies of the final channel and the upper band edge;

DS Duplex spacing (fn’ - fn).

**6760 MHz**

**7125**

328.5MHz

3 MHz

4 x 3.5 MHz

4 x 3.5 MHz

5.5

MHz

a) 3.5 MHz channels

c) 0.5 MHz channels

328.5 MHz

 3

 MHz

28 x 0.5 MHz

28 x 0.5 MHz

5.5

MHz

328.5 MHz

3

MHz

56 x 0.25 MHz

56 x 0.25 MHz

5.5

MHz

e) 0.025 MHz channels

328.5 MHz

3

MHz

560 x 0.025 MHz

560 x 0.025 MHz

5.5

MHz

d) 0.25 MHz channels

328.5 MHz

3

MHz

8 x 1.75 MHz

5.5

MHz

8 x 1.75 MHz

b) 1.75 MHz channels

1. Occupied spectrum
	1. Implementation of narrow channels and 30 MHz channels
		1. Derivation of radio frequency channel

The radio frequency channel arrangement for carrier spacings of 3.5 MHz, 1.75 MHz, 0.5 MHz, 0.25 MHz and 0.025 MHz shall be derived as follows:

Let

f0 be the frequency (MHz) of the center of the band of frequencies occupied, f0 = 6 950 MHz,

fn be the center frequency (MHz) of one radio-frequency channel in the lower half of the band,

fn’ be the center frequency (MHz) of one radio-frequency channel in the upper half of the band,

then the frequencies (MHz) of individual channels are expressed by the following relationships:

a) for systems with a carrier spacing of 3.5 MHz:

lower half of the band: fn = f0 – 175.25 + 3.5 n

upper half of the band: fn’ = f0 + 164.75 + 3.5 n where n = 1, 2.

b) for systems with a carrier spacing of 1.75 MHz:

lower half of the band: fn = f0 – 174.375 + 1.75 n

upper half of the band: fn’ = f0 + 165.625 + 1.75 n where n = 1, 2, 3, 4.

c) for systems with a carrier spacing of 0.5 MHz:

lower half of the band: fn = f0 – 173.75 + 0.5 n

upper half of the band: fn’ = f0 + 166.25 + 0.5 n where n = 1, 2…..9, 14.

d) for systems with a carrier spacing of 0.25 MHz:

lower half of the band: fn = f0 – 173.625 + 0.25 n

upper half of the band: fn’ = f0 + 166.375 + 0.25 n where n = 1, 2…..27, 28.

e) for systems with a carrier spacing of 0.025 MHz:

lower half of the band: fn = f0 – 173.5125 + 0.025 n

upper half of the band: fn’ = f0 + 166.4875 + 0.025 n where n = 1, 2…..199, 280.

* + 1. Calculated parameters according to Recommendation ITU-R F.746

Table 3: Calculated parameters according to Recommendation ITU-R F.746

| **XS****(MHz)** | **n** | **f1****(MHz)** | **fn****(MHz)** | **f1’****(MHz)** | **fn’****(MHz)** | **YS (MHz)** | **DS (MHz)** |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 3.5 | 1.2 | 6778.25 | 6781.75 | 7118.25 | 7121.75 | 336.5 | 340 |
| 1.75 | 1…4 | 6777.375 | 6782.625 | 7117.375 | 7122.625 | 334.75 | 340 |
| 0.5 | 1…14 | 6776.75 | 6783.25 | 7116.75 | 7123.25 | 333.5 | 340 |
| 0.25 | 1…28 | 6776.625 | 6783.375 | 7116.625 | 7123.375 | 333.25 | 340 |
| 0.025 | 1...280 | 6776.5125 | 6783.4875 | 7116.5125 | 7123.4875 | 333.025 | 340 |

XS Separation between centre frequencies of adjacent channels;

YS Separation between centre frequencies of the closest go and return channels;

Z1S Separation between the lower band edge and the centre frequency of the first channel;

Z2S Separation between centre frequencies of the final channel and the upper band edge;

DS Duplex spacing (fn’ - fn).

**6775 MHz**

**7125 MHz**

c) 0.5 MHz channels

333 MHz

1.5

MHz

14 x 0.5 MHz

14 x 0.5 MHz

1.5

MHz

d) 0.25 MHz channels

333 MHz

1.5

MHz

28 x 0.25 MHz

28 x 0.25 MHz

1.5

MHz

333 MHz

1.5

MHz

280 x 0.025 MHz

280 x 0.025 MHz

1.5

MHz

e) 0.025 MHz channels

b) 1.75 MHz channels

333 MHz

1.5

MHz

4 x 1.75 MHz

1.5

MHz

4 x 1.75 MHz

333 MHz

1.5

MHz

2 \* 3.5 MHz

1.5

MHz

2 \* 3.5 MHz

a) 3.5 MHz channels

1. Occupied spectrum
2. iLLUSTRATIONS OF THE IMPLEMENTATION OF NARROW CHANNELS in the 6 GHz band

**8x40**

**8x40**

**8x29.65**

**10.5 MHz**

**14 MHz**

**10.5 MHz**

**14 MHz**

**8x29.65**

**5925**

**6425**

**7125**

5.375 MHz

2.17 MHz

2.17 MHz

4.938 MHz

4.947 MHz

3 MHz

3 MHz

5.5 MHz

5.5 MHz

**Current L6 GHz plan**

**Current U6 GHz plan**

**Proposed plans to implement narrow channels**

**1**

**2**

1. Illustration of implementation of narrow channels in the lower part of the 6 GHz band and 40 MHz channels in the U6 band

**11x30**

**11x30**

**8x29.65**

**10.5 MHz**

**7 MHz**

**10.5 MHz**

**7 MHz**

**8x29.65**

**5925**

**6425**

**7125**

5.375 MHz

2.17 MHz

2.17 MHz

4.938 MHz

9.947 MHz

1.5 MHz

1.5 MHz

1.5 MHz

1.5 MHz

**Current L6 GHz plan**

**Current U6 GHz plan**

**Proposed plans to implement narrow channels**

**1**

**2 bis**

1. Illustration of implementation of narrow channels in the lower part of the 6 GHz band and 30 MHz channels in the U6 band
2. list of reference
3. ERC Recommendation 14-01: radio-frequency channel arrangements for high capacity analogue and digital radio-relay systems operating in the band 5925 -6425 MHz
4. ERC Recommendation 14-02: radio-frequency channel arrangements for high, medium and low capacity digital fixed service systems operating in the band 6425-7125 MHz
5. ECC Report 215: Assessment of the technical feasibility of introducing very narrow channel spacing in some existing plans, in guard bands and center gaps of FWS channel arrangement at 6 GHz and
10 GHz