Radio Interface Specification Template
RIS implementation of ECC/REC/(08)01 on use of the band 5855-5875 MHz for non-safety related Road Intelligent Transport
(approved by WG FM#111)
This RIS implementation is limited to frequency arrangements for ITS in the 5855-5875 MHz bands 
Table 1: Normative Part
	Nr
	Parameter
	Description
	Comments

	1
	Radiocommunication
Service
	Mobile Service
	

	2
	Application
	Intelligent Transport Systems (ITS)
	ITS non-safety related communication includes Infrastructure to Vehicle (I2V) communication and Vehicle to Vehicle (V2V) communications between ITS stations in highly dynamic ad-hoc networks.

	3
	Frequency band
	5855-5875 MHz
	5855-5875 MHz is on a non-exclusive basis for non-safety related Road ITS. 

	4
	Channelling
	The frequency arrangement is based on a block size of 10 MHz starting at the lower edge of the band, at 5855 MHz. Two blocks can be combined to one contiguous 20 MHz channel.
	Channel bandwidth may be lower than 10 MHz.

	5
	Modulation / 
Occupied bandwidth 
	Not specified
	Technology neutral approach

	6
	Direction / 
Separation
	Not applicable 
	

	7
	Transmit power / Power density
	spectral power density for ITS devices is limited to 23 dBm/MHz e.i.r.p.; 
transmit power shall not exceed 33 dBm e.i.r.p. 
	Transmit Power Control (TPC) should be able to reduce the total power from its maximum to 3 dBm e.i.r.p.

	8
	Channel access and occupation rules
	Not specified
	

	9
	Authorisation regime
	General authorisation
	No registration and/or notification is required (commonly known as “licence exempt”).

	10
	Additional essential requirements according to Art. 3.3 of Radio Equipment Directive 2014/53/EU
	None
	

	11
	Frequency planning assumptions
	ECC Report 101, ECC Report 228 and ECC Report 290
	Unwanted emission limits apply for the protection of other systems in adjacent bands. Equivalent mitigation techniques, as defined in the relevant harmonised European standard ETSI EN 302 571 may also be used.


Table 2: Informative Part
	Nr
	Parameter
	Description
	Comments

	12
	Planned changes
	
	

	13
	Reference
	ECC/REC/(08)01
EN 302 571 
Decision (EU) 2025/105
	

	14
	Notification number 
	
	

	15
	Remarks 
	Abbreviation
e.i.r.p. equivalent isotropically radiated power
	



