Radio Interface Specification Template
RIS implementation of ECC/DEC/(20)01 on the harmonised use of the frequency band 5945-6425 MHz for Wireless Access Systems including Radio Local Area Networks (WAS/RLAN) 
(approved by WG FM#111)
This RIS implementation is limited to harmonised use of the 5945-6425 MHz frequency band for Wireless Systems including Radio Local Area Networks  
Table 1: Normative Part
	Nr
	Parameter
	Description
	Comments

	1
	Radiocommunication
Service
	Mobile Service
	

	2
	Application
	RLAN
	Type of devices: 
Low Power Indoor (LPI) devices
Very low Power (VLP) devices

	3
	Frequency band
	5945-6425 MHz 
	

	4
	Channelling
	Narrowband devices operate in channels bandwidth below 20 MHz. 
Wideband devices operate in channels bandwidth above or equal to 20 MHz.
	

	5
	Modulation / 
Occupied bandwidth 
	Not specified
	Technology neutral approach

	6
	Direction / 
Separation
	Not applicable 
	

	7
	Transmit power / Power density
	· LPI: maximum mean e.i.r.p. for in-band emissions is limited to 23 dBm and maximum spectral power density for in-band emissions is limited to 10 dBm/MHz e.i.r.p. 
VLP: maximum mean e.i.r.p. for in-band emissions is limited to 14 dBm. Maximum spectral power density for in-band emissions is limited to 1 dBm/MHz e.i.r.p. for broadband devices and limited to 10 dBm/MHz e.i.r.p. for narrow band devices. 
	VLP Narrowband devices also require a frequency hopping mechanism based on at least 15 hop channels to operate at a PSD value above 1 dBm/MHz.


	8
	Channel access and occupation rules
	An adequate spectrum sharing mechanism shall be implemented.  
	

	9
	Authorisation regime
	General authorisation
	5945-6425 MHz is on a non-exclusive, non-interference and non-protected basis. 
No registration and/or notification is required (commonly known as “licence exempt”).

	10
	Additional essential requirements according to Art. 3.3 of Radio Equipment  Directive 2014/53/EU
	None
	

	11
	Frequency planning assumptions
	Specific unwanted emission limits apply for the protection of Urban Rail systems (such as CBTC) below 5935 MHz: 
LPI: Maximum mean e.i.r.p. density for out-of-band emissions below 5935 MHz of -22 dBm/MHz
VLP: Maximum mean e.i.r.p. density for out-of-band emissions below 5935 MHz of  -37 dBm/MHz (Note: VLP devices shall first attempt to select a frequency block above 6105 MHz when initiating a communication session. Alternatively, where no such mechanism is implemented, then a maximum mean e.i.r.p. density for out-of-band emissions of -45 dBm/MHz below 5935 MHz applies.) (See ECC/DEC(20)01, annex A1.2)
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Table 2: Informative Part
	Nr
	Parameter
	Description
	Comments

	12
	Planned changes
	
	

	13
	Reference
	Decision (EU) 2025/913 
ECC/DEC/(20)01
EN 303 687
	

	14
	Notification number 
	
	

	15
	Remarks 
	Abbreviation
e.i.r.p. equivalent isotropically radiated power
	



