Radio Interface Specification Template
RIS implementation of ERC/DEC/(01)11 “Harmonised frequencies, technical characteristics and exemption from individual licensing of short range devices used for Flying Model control operating in the frequency band 34.995-35.225 MHz”
(approved by WG FM#113)
Foreword
The ECC has decided that RIS implementations of ECC deliverables should be uploaded to the ECO website in order to help administrations fill out the EFIS database.
Completing this table has two benefits for CEPT Administrations. Foremost, it provides a template for any nation Interface Requirement that may be provided to the European Commission or used as part of the national regulation/authorisation on use. It additionally provides the necessary information for the ECC Deliverable to be correctly referenced in the EFIS database and ECO Documentation Database (DocDB).
There is a guidance document for the template[footnoteRef:2] which was updated for RIS information under the RE-D. [2: Notification of radio interface specifications and radio equipment classes - Notification template and guidance (https://ec.europa.eu/docsroom/documents/26844)
] 

Note; the EU defined Application term may differ from the ECC Defined Application term.  If this is the case, please notify the ECO of the correct ECC term when developing this RIS information.
This RIS implementation is limited to frequency arrangements for short range devices used for Flying model control in the 34.995-35.225 MHz bands


Table 1: Normative Part
	Nr
	Parameter
	Description
	Comments

	1
	Radiocommunication
Service
	Not applicable
	

	2
	Application
	Flying model control
	

	3
	Frequency band
	34.995-35.225 MHz
	

	4
	Channelling
	Not specified
	

	5
	Modulation / 
Occupied bandwidth 
	≤ 10 kHz
	

	6
	Direction / 
Separation
	Not specified
	

	7
	Transmit power / Power density
	100 mW e.r.p.
	

	8
	Channel access and occupation rules
	Not specified
	

	9
	Authorisation regime
	General authorisation
	No registration and/or notification is required (commonly known as “licence exempt”).

	10
	Additional essential requirements 
	None
	

	11
	Frequency planning assumptions
	Not applicable
	


Table 2: Informative Part
	Nr
	Parameter
	Description
	Comments

	12
	Planned changes
	
	

	13
	Reference
	ERC/DEC/(01)11, EN 300 220
	

	14
	Notification number 
	
	

	15
	Remarks 
	
	ITU‐R RR Article number 4.4



